Channel in a box

Device Control Protocol

Version 1.5

* **Document Revision History**

|  |  |  |  |
| --- | --- | --- | --- |
| **Version** | **Date** | **Changes** | **Writer** |
| 1.0 | 02-10-2017 | First document for general distribution | Sangbong, Lee |
| 1.1 | 02-28-2017 | Add MCS(Master Switch) protocol | Sangbong, Lee |
| 1.2 | 06-27-2017 | Add get device number function  Modify MCS crosspoint take function  Add MCS key functions | Sangbong, Lee |
| 1.3 | 07-08-2019 | Add "command" to the beginning of every response packet. | Sangbong, Lee |
| 1.4 | 07-22-2019 | * Add MCS functions “get\_status\_key” assign key to bus response | Sangbong, Lee |
| 1.5 | 07-23-2019 | * Add MCS functions “key\_assign assign key to bus “get\_key\_assign” get assigned key to bus * Modify MCS function “get\_crosspoint\_take” bus parameter delete “get\_status\_key” -> “get\_key\_take” * Add all play device function “get\_rate” get play rate | Sangbong, Lee |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |

1. **Introduction**

Defines a protocol for a device to be used in a channel in a box (CIB).

CIB Device consists of Video Encoder / Decoder, CG (Cut & Page), Sequence CG, Scroll CG, Logo, Closed Caption & Sub Title, MCS and describes control protocol for each device in this document.

1. **Interface System Overview**

* The protocol is based on JSON
* Confirming to UDP & RS-422
* Data is transmitted asynchronously, with data exchange between devices.
* Standard transmission UDP port on see the below :

Video Encoder/Decoder : 1000 ~ 1099

CG (Cut & Page) : 1100 ~ 1199

Sequence CG : 1200 ~ 1299

Scroll CG : 1300 ~ 1399

Logo : 1400 ~ 1499

Closed Caption & Sub Title : 1500 ~ 1599

Master Control Switch : 2000

1. **JSON Protocol Format**

* Command Default  
  {  
   “command” : “”   
  }
* Response Default  
  If success  
  {  
   “command” : “”  
   “response” : “success”  
  }  
    
  If fail  
  {  
   “command” : “”  
   “response” : “fail”,  
   “errorcode” : 0  
  }
* Depending on the type of command, the convention for JSON objects is different.
* Response also define additional JSON objects depending on the type of command.
* The command is classified according to the mode of operation. See the below :  
  System Control  
  Immediate Control  
  Preset/Select Control  
  Sens Request
* It should be noted that the response of all commands except “Sense Request” is not a result of the command but a command that is normally received.

1. **Command**
2. **Command Table (Video Encoder/Decoder)**

|  |  |  |  |
| --- | --- | --- | --- |
| **Command** | | **Response** | |
| **JSON Object** | **Description** | **JSON Object** | **Description** |
| **System Control** | | | |
| open | Device open | Success | Command success |
| close | Device close | Success | Command success |
| **Immediate Control** | | | |
| stop | Stop | Success | Command success |
| play | Play or Record | Success | Command success |
| pause | Pause | Success | Command success |
| set\_rate | Set play rate | Success | Command success |
| set\_timecode | Go to timecode position | Success | Command success |
| **Preset/Select Control** | | | |
| play\_cue | Play cue | Success | Command success |
| play\_cue\_data | Play cue & Start & Duration | Success | Command success |
| record\_cue | Record cue | Success | Command success |
| record\_cue\_data | Record cue & Duration | Success | Command success |
| **Sense Request** | | | |
| get\_device\_no | Get device number | Success & Data | Command success & device number data |
| get\_status | Get device status | Success & Data | Command success & status data |
| get\_rate | Get play rate | Success & Data | Command success & play rate data |
| get\_timecode | Get timecode | Success & Data | Command success & timecode data |

1. **Command Table (CG – Cut & Page)**

|  |  |  |  |
| --- | --- | --- | --- |
| **Command** | | **Response** | |
| **JSON Object** | **Description** | **JSON Object** | **Description** |
| **System Control** | | | |
| open | Device open | Success | Command success |
| close | Device close | Success | Command success |
| **Immediate Control** | | | |
| stop | Stop | Success | Command success |
| play | Play | Success | Command success |
| set\_page | Go to CG cut page | Success | Command success |
| **Preset/Select Control** | | | |
| play\_cue | Play cue | Success | Command success |
| template\_data | Set template data | Success | Command success |
| **Sense Request** | | | |
| get\_device\_no | Get device number | Success & Data | Command success & device number data |
| get\_status | Get device status | Success & Data | Command success & status data |

1. **Command Table (Sequence CG)**

|  |  |  |  |
| --- | --- | --- | --- |
| **Command** | | **Response** | |
| **JSON Object** | **Description** | **JSON Object** | **Description** |
| **System Control** | | | |
| open | Device open | Success | Command success |
| close | Device close | Success | Command success |
| **Immediate Control** | | | |
| stop | Stop | Success | Command success |
| play | Play | Success | Command success |
| pause | Pause | Success | Command success |
| set\_rate | Set play rate | Success | Command success |
| set\_timecode | Go to timecode position | Success | Command success |
| **Preset/Select Control** | | | |
| play\_cue | Play Cue – Sequence name | Success | Command success |
| play\_cue\_data | Play Cue & Start & Duration | Success | Command success |
| **Sense Request** | | | |
| get\_device\_no | Get device number | Success & Data | Command success & device number data |
| get\_status | Get device status | Success & Data | Command success & status data |
| get\_rate | Get play rate | Success & Data | Command success & play rate data |
| get\_timecode | Get timecode | Success & Data | Command success & timecode data |

1. **Command Table (Scroll CG)**

|  |  |  |  |
| --- | --- | --- | --- |
| **Command** | | **Response** | |
| **JSON Object** | **Description** | **JSON Object** | **Description** |
| **System Control** | | | |
| open | Device open | Success | Command success |
| close | Device close | Success | Command success |
| **Immediate Control** | | | |
| stop | Scroll Stop | Success | Command success |
| play | Play on scroll | Success | Command success |
| pause | Pause | Success | Command success |
| set\_rate | Set scroll rate | Success | Command success |
| **Preset/Select Control** | | | |
| play\_cue | Play Cue – Scroll template name | Success | Command success |
| set\_data | Set scroll data | Success | Command success |
| **Sense Request** | | | |
| get\_device\_no | Get device number | Success & Data | Command success & device number data |
| get\_status | Get device status | Success & Data | Command success & status data |
| get\_rate | Get scroll rate | Success & Data | Command success & scroll rate data |

1. **Command Table (Logo)**

|  |  |  |  |
| --- | --- | --- | --- |
| **Command** | | **Response** | |
| **JSON Object** | **Description** | **JSON Object** | **Description** |
| **System Control** | | | |
| open | Device open | Success | Command success |
| close | Device close | Success | Command success |
| **Immediate Control** | | | |
| stop | Stop | Success | Command success |
| play | Play | Success | Command success |
| **Preset/Select Control** | | | |
| play\_cue | Play Cue – Logo name | Success | Command success |
| **Sense Request** | | | |
| get\_device\_no | Get device number | Success & Data | Command success & device number data |
| get\_status | Get device status | Success & Data | Command success & status data |

1. **Command Table (Closed Caption & Sub Title)**

|  |  |  |  |
| --- | --- | --- | --- |
| **“Command” JSON Object** | | **“Response” JSON Object** | |
| **JSON Value** | **Description** | **JSON Value** | **Description** |
| **System Control** | | | |
| open | Device open | Success | Command success |
| close | Device close | Success | Command success |
| **Immediate Control** | | | |
| stop | Stop | Success | Command success |
| play | Play | Success | Command success |
| pause | Pause | Success | Command success |
| set\_on | Set screen display on or off | Success | Command success |
| **Preset/Select Control** | | | |
| play\_cue | Play Cue – preset or smi | Success | Command success |
| play\_cue\_data | Play Cue & Start & Duration | Success | Command success |
| **Sense Request** | | | |
| get\_device\_no | Get device number | Success & Data | Command success & device number data |
| get\_status | Get device status | Success & Data | Command success & status data |
| get\_timecode | Get timecode | Success & Data | Command success & timecode data |

1. **Command Table (MCS – Master Control Switch)**

|  |  |  |  |
| --- | --- | --- | --- |
| **“Command” JSON Object** | | **“Response” JSON Object** | |
| **JSON Value** | **Description** | **JSON Value** | **Description** |
| **System Control** | | | |
| open | Device open | Success | Command success |
| close | Device close | Success | Command success |
| **Immediate Control** | | | |
| next\_transition | Next transition | Success | Command success |
| start\_transition | Start transition | Success | Command success |
| crosspoint\_take | Crosspoint take | Success | Command success |
| key\_take | Key take | Success | Command success |
| **Preset/Select Control** | | | |
| set\_transition\_type | Set transition type | Success | Command success |
| set\_transition\_rate | Set transition rate | Success | Command success |
| set\_enable\_key | Set enable key | Success | Command success |
| **Sense Request** | | | |
| get\_transition\_type | Get transition type | Success & Data | Command success & transition type data |
| get\_transition\_rate | Get transition rate | Success & Data | Command success & transition rate data |
| get\_crosspoint\_take | Get crosspoint take | Success & Data | Command success & crosspoint take data |
| get\_enable\_key | Get enable key | Success | Command success & key enable data. |
| get\_status\_key | Get key status | Success & Data | Command success & key status data |
| get\_status | Get device status | Success & Data | Command success & status data |

1. **Command Description**
2. **Video Encoder/Decoder**

**System Control**

* **open**Open to use device.  
  No other commands can be executed before this command is executed.  
    
  {   
   “command” : “open”  
  }
* **close**  
  Close the device.  
  No other commands can be executed after this command.  
    
  {   
   “command” : “close”  
  }

**Immediate Control**

* **stop**The [stop] command stops playback or recording.  
    
  {   
   “command” : “stop”  
  }
* **play**Start playback or recording.  
  If the decoder in PAUSE state, the [play] command start playback or recording at current position.
* Play Cue before you start playback.
* Record Cue before you start record.

{   
 “command” : “play”  
}

* **pause**The [pause] command pause playback or recording.  
  If the decoder in PLAY or PLAY CUE state, the [pause] command causes the currently playing ID to pause and display a still video frame.  
  If the encoder in RECORD or RECORD CUE state, the PAUSE command causes the currently recording ID to pause.  
    
  {   
   “command” : “pause”  
  }
* **set\_rate**Specifies the playback speed  
  If it is positive, it is forward.  
  If it is negative, it is rewind.  
  If it is 0, it is pause.  
  This command can be used to implement the Jog & Shuttle function.

|  |  |  |  |
| --- | --- | --- | --- |
| **JSON Object** | **JSON Value** | **Value Type** | **Description** |
| command | set\_rate | String |  |
| rate | 0 | Number (float) | 0 : pause  Greater then 0 : forward play  Less then 0 : rewind play |

{   
 “command” : “set\_rate”,  
 “rate” : 0  
}

* **set\_timecode**If playback is in progress, position the video in timecode.  
  If the time code is larger than the video duration, it moves to the back of the video.

|  |  |  |  |
| --- | --- | --- | --- |
| **JSON Object** | **JSON Value** | **Value Type** | **Description** |
| command | set\_timecode | String |  |
| timecode | 00:00:00:00 | String | Timecode (DF & NDF) |

{   
 “command” : “set\_timecode”,  
 “timecode” : “00:00:00:00”  
}

**Preset/Select Control**

* **play\_cue**The [play\_cue] command prepares for playback.  
  If the ID is not found, an error occurs and state returns STOP.  
  When the CUE is complete, the CUE-DONE flag is set in status.

|  |  |  |  |
| --- | --- | --- | --- |
| **JSON Object** | **JSON Value** | **Value Type** | **Description** |
| command | play\_cue | String |  |
| id | id | String | Video material id |

{   
 “command” : “play\_cue”,  
 “id” : “id”  
}

* **play\_cue\_data**Performs similar to [play\_cue].  
  In addition, you can specify playback start timecode and playback duration.

|  |  |  |  |
| --- | --- | --- | --- |
| **JSON Object** | **JSON Value** | **Value Type** | **Description** |
| command | play\_cue\_data | String |  |
| id | id | String | Video material id |
| start | 00:00:00:00 | String | Playback start timecode |
| duration | 00:59:59:29 | String | Playback duration timecode |

{   
 “command” : “play\_cue\_data”,  
 “id” : “id”,  
 “start” : “00:00:00:00”,  
 “duration” : “00:59:59:29”  
}

* **record\_cue**The [record\_cue] command prepares for record.  
  If there is an existing ID, it overwrites it, and immediately the ID has a length of 0.  
  When the CUE is complete, the CUE-DONE flag is set in status.

|  |  |  |  |
| --- | --- | --- | --- |
| **JSON Object** | **JSON Value** | **Value Type** | **Description** |
| command | record\_cue | String |  |
| id | id | String | Video material id |

{   
 “command” : “record\_cue”,  
 “id” : “id”  
}

* **record\_cue\_data**Performs similar to [record\_cue].  
  In addition, you can specify record duration.  
  When recording is done for the specified duration, it stops automatically.

|  |  |  |  |
| --- | --- | --- | --- |
| **JSON Object** | **JSON Value** | **Value Type** | **Description** |
| command | play\_cue\_data | String |  |
| id | id | String | Video material id |
| duration | 00:59:59:29 | String | Playback duration timecode |

{   
 “command” : “play\_cue\_data”,  
 “id” : “id”,  
 “duration” : “00:59:59:29”  
}

**Sense Request**

* **get\_device\_no**The [get\_device\_no] command get device number.  
    
  {   
   “command” : “get\_device\_no”  
  }  
    
  **Response**

|  |  |  |  |
| --- | --- | --- | --- |
| **JSON Object** | **JSON Value** | **Value Type** | **Description** |
| command | get\_device\_no | String |  |
| response | success | String | Success or Fail |
| no | 0 | Number | Get PCS the set device number. |

* **get\_status**The [get\_status] command get device status.  
    
  {   
   “command” : “get\_status”  
  }  
    
  **Response**

|  |  |  |  |
| --- | --- | --- | --- |
| **JSON Object** | **JSON Value** | **Value Type** | **Description** |
| command | get\_status | String |  |
| response | success | String | Success or Fail |
| * status idle cueing cue\_done play pause | true  false  false  false  false | Boolean  Boolean  Boolean  Boolean  Boolean | Not doing anything or stopped  Preparing play or record  Completed prepare play or record  Playing  Paused |

* **get\_rate**The [get\_rate] command get current play rate.  
    
  {   
   “command” : “get\_rate”  
  }  
    
  **Response**

|  |  |  |  |
| --- | --- | --- | --- |
| **JSON Object** | **JSON Value** | **Value Type** | **Description** |
| command | get\_timecode | String |  |
| response | success | String | Success or Fail |
| rate | 0 | Number (float) | 0 : pause  Greater then 0 : forward play  Less then 0 : rewind play |

* **get\_timecode**The [get\_timecode] command get current timecode.  
    
  {   
   “command” : “get\_timecode”  
  }  
    
  **Response**

|  |  |  |  |
| --- | --- | --- | --- |
| **JSON Object** | **JSON Value** | **Value Type** | **Description** |
| command | get\_timecode | String |  |
| response | success | String | Success or Fail |
| timecode | 00:00:00:00 | String |  |

1. **CG – Cut & Page**

**System Control**

* **open**Open to use device.  
  No other commands can be executed before this command is executed.  
    
  {   
   “command” : “open”  
  }
* **close**  
  Close the device.  
  No other commands can be executed after this command.  
    
  {   
   “command” : “close”  
  }

**Immediate Control**

* **stop**The [stop] command stops playback.  
    
  {   
   “command” : “stop”  
  }
* **play**Start playback CG.
* Play Cue before you start playback.

{   
 “command” : “play”  
}

* **set\_page**If there are several cut pages, specify the page number.  
  If playback is in progress, specify the page number then immediately display on screen.

|  |  |  |  |
| --- | --- | --- | --- |
| **JSON Object** | **JSON Value** | **Value Type** | **Description** |
| command | set\_page | String |  |
| page | 0 | Number | Start page number of 0 |

{   
 “command” : “set\_page”,  
 “page” : 0  
}

**Preset/Select Control**

* **play\_cue**The [play\_cue] command prepares for playback.  
  If the ID is not found, an error occurs and state returns STOP.  
  When the CUE is complete, the CUE-DONE flag is set in status.

|  |  |  |  |
| --- | --- | --- | --- |
| **JSON Object** | **JSON Value** | **Value Type** | **Description** |
| command | play\_cue | String |  |
| id | id | String | CG template id |

{   
 “command” : “play\_cue”,  
 “id” : “id”  
}

* **set\_data**Set the data of the cued template.  
  Template data is separate JSON array.

|  |  |  |  |
| --- | --- | --- | --- |
| **JSON Object** | **JSON Value** | **Value Type** | **Description** |
| command | set\_data | String |  |
| data | data | String array | Template data, JSON array |

{   
 “command” : “set\_data”,  
 “data” : [  
 “data1”,  
 “data2”,  
 “data3”  
 ]  
}

**Sense Request**

* **get\_device\_no**The [get\_device\_no] command get device number.  
    
  {   
   “command” : “get\_device\_no”  
  }  
    
  **Response**

|  |  |  |  |
| --- | --- | --- | --- |
| **JSON Object** | **JSON Value** | **Value Type** | **Description** |
| command | get\_device\_no | String |  |
| response | success | String | Success or Fail |
| no | 0 | Number | Get PCS the set device number. |

* **get\_status**The [get\_status] command get device status.  
    
  {   
   “command” : “get\_status”  
  }  
    
  **Response**

|  |  |  |  |
| --- | --- | --- | --- |
| **JSON Object** | **JSON Value** | **Value Type** | **Description** |
| command | get\_status | String |  |
| response | success | String | Success or Fail |
| * status idle cueing cue\_done play page | true  false  false  false  0 | Boolean  Boolean  Boolean  Boolean  Number | Not doing anything or stopped  Preparing play  Completed prepare play  Playing  Paused |

1. **Sequence CG**

**System Control**

* **open**Open to use device.  
  No other commands can be executed before this command is executed.  
    
  {   
   “command” : “open”  
  }
* **close**  
  Close the device.  
  No other commands can be executed after this command.  
    
  {   
   “command” : “close”  
  }

**Immediate Control**

* **stop**The [stop] command stops playback.  
    
  {   
   “command” : “stop”  
  }
* **play**Start playback.  
  If the decoder in PAUSE state, the [play] command start playback at current position.
* Play Cue before you start playback.

{   
 “command” : “play”  
}

* **pause**The [pause] command pause playback.  
  If the device in PLAY or PLAY CUE state, the [pause] command causes the currently playing ID to pause and display a still video frame.  
    
  {   
   “command” : “pause”  
  }
* **set\_rate**Specifies the playback speed  
  If it is positive, it is forward.  
  If it is negative, it is rewind.  
  If it is 0, it is pause.  
  This command can be used to implement the Jog & Shuttle function.

|  |  |  |  |
| --- | --- | --- | --- |
| **JSON Object** | **JSON Value** | **Value Type** | **Description** |
| command | set\_rate | String |  |
| rate | 0 | Number (float) | 0 : pause  Greater then 0 : forward play  Less then 0 : rewind play |

{   
 “command” : “set\_rate”,  
 “rate” : 0  
}

* **get\_rate**The [get\_rate] command get current play rate.  
    
  {   
   “command” : “get\_rate”  
  }  
    
  **Response**

|  |  |  |  |
| --- | --- | --- | --- |
| **JSON Object** | **JSON Value** | **Value Type** | **Description** |
| command | get\_timecode | String |  |
| response | success | String | Success or Fail |
| rate | 0 | Number (float) | 0 : pause  Greater then 0 : forward play  Less then 0 : rewind play |

* **set\_timecode**If playback is in progress, position the video in timecode.  
  If the time code is larger than the video duration, it moves to the back of the video.

|  |  |  |  |
| --- | --- | --- | --- |
| **JSON Object** | **JSON Value** | **Value Type** | **Description** |
| command | set\_timecode | String |  |
| timecode | 00:00:00:00 | String | Timecode (DF & NDF) |

{   
 “command” : “set\_timecode”,  
 “timecode” : “00:00:00:00”  
}

**Preset/Select Control**

* **play\_cue**The [play\_cue] command prepares for playback.  
  If the ID is not found, an error occurs and state returns STOP.  
  When the CUE is complete, the CUE-DONE flag is set in status.

|  |  |  |  |
| --- | --- | --- | --- |
| **JSON Object** | **JSON Value** | **Value Type** | **Description** |
| command | play\_cue | String |  |
| id | id | String | Sequence id or name |

{   
 “command” : “play\_cue”,  
 “id” : “id”  
}

* **play\_cue\_data**Performs similar to [play\_cue].  
  In addition, you can specify playback start timecode and playback duration.

|  |  |  |  |
| --- | --- | --- | --- |
| **JSON Object** | **JSON Value** | **Value Type** | **Description** |
| command | play\_cue\_data | String |  |
| id | id | String | Sequence id or name |
| start | 00:00:00:00 | String | Playback start timecode |
| duration | 00:59:59:29 | String | Playback duration timecode |

{   
 “command” : “play\_cue\_data”,  
 “id” : “id”,  
 “start” : “00:00:00:00”,  
 “duration” : “00:59:59:29”  
}

**Sense Request**

* **get\_device\_no**The [get\_device\_no] command get device number.  
    
  {   
   “command” : “get\_device\_no”  
  }  
    
  **Response**

|  |  |  |  |
| --- | --- | --- | --- |
| **JSON Object** | **JSON Value** | **Value Type** | **Description** |
| command | get\_device\_no | String |  |
| response | success | String | Success or Fail |
| no | 0 | Number | Get PCS the set device number. |

* **get\_status**The [get\_status] command get device status.  
    
  {   
   “command” : “get\_status”  
  }  
    
  **Response**

|  |  |  |  |
| --- | --- | --- | --- |
| **JSON Object** | **JSON Value** | **Value Type** | **Description** |
| command | get\_status | String |  |
| response | success | String | Success or Fail |
| * status idle cueing cue\_done play pause | true  false  false  false  false | Boolean  Boolean  Boolean  Boolean  Boolean | Not doing anything or stopped  Preparing play  Completed prepare play  Playing  Paused |

* **get\_timecode**The [get\_timecode] command get current timecode.  
    
  {   
   “command” : “get\_timecode”  
  }  
    
  **Response**

|  |  |  |  |
| --- | --- | --- | --- |
| **JSON Object** | **JSON Value** | **Value Type** | **Description** |
| command | get\_timecode | String |  |
| response | success | String | Success or Fail |
| timecode | 00:00:00:00 | String |  |

1. **Scroll CG**

**System Control**

* **open**Open to use device.  
  No other commands can be executed before this command is executed.  
    
  {   
   “command” : “open”  
  }
* **close**  
  Close the device.  
  No other commands can be executed after this command.  
    
  {   
   “command” : “close”  
  }

**Immediate Control**

* **stop**The [stop] command stops scroll.  
    
  {   
   “command” : “stop”  
  }
* **play**Start playback scroll.
* Play Cue before you start playback scroll.

{   
 “command” : “play”  
}

* **pause**The [pause] command pause playback scroll.  
  If the device in PLAY or PLAY CUE state, the [pause] command causes the currently scrolling template ID to pause and display a still scroll.  
    
  {   
   “command” : “pause”  
  }
* **set\_rate**Specifies the playback scroll speed  
  If it is positive, it is forward.  
  If it is negative, it is rewind.  
  If it is 0, it is pause.  
  This command can be used to implement the Jog & Shuttle function.

|  |  |  |  |
| --- | --- | --- | --- |
| **JSON Object** | **JSON Value** | **Value Type** | **Description** |
| command | set\_rate | String |  |
| rate | 0 | Number (float) | 0 : pause  Greater then 0 : forward scroll  Less then 0 : rewind scroll |

{   
 “command” : “set\_rate”,  
 “rate” : 0  
}

**Preset/Select Control**

* **play\_cue**The [play\_cue] command prepares for playback scroll.  
  If the template ID is not found, an error occurs and state returns STOP.  
  When the CUE is complete, the CUE-DONE flag is set in status.

|  |  |  |  |
| --- | --- | --- | --- |
| **JSON Object** | **JSON Value** | **Value Type** | **Description** |
| command | play\_cue | String |  |
| id | id | String | Template ID |

{   
 “command” : “play\_cue”,  
 “id” : “id”  
}

* **set\_data**Set the data of the cued scroll template.  
  Template data is separate JSON array.

|  |  |  |  |
| --- | --- | --- | --- |
| **JSON Object** | **JSON Value** | **Value Type** | **Description** |
| command | set\_data | String |  |
| data | data | String array | Template data, JSON array |

{   
 “command” : “set\_data”,  
 “data” : [  
 “data1”,  
 “data2”,  
 “data3”  
 ]  
}

**Sense Request**

* **get\_device\_no**The [get\_device\_no] command get device number.  
    
  {   
   “command” : “get\_device\_no”  
  }  
    
  **Response**

|  |  |  |  |
| --- | --- | --- | --- |
| **JSON Object** | **JSON Value** | **Value Type** | **Description** |
| command | get\_device\_no | String |  |
| response | success | String | Success or Fail |
| no | 0 | Number | Get PCS the set device number. |

* **get\_status**The [get\_status] command get device status.  
    
  {   
   “command” : “get\_status”  
  }  
    
  **Response**

|  |  |  |  |
| --- | --- | --- | --- |
| **JSON Object** | **JSON Value** | **Value Type** | **Description** |
| command | get\_status | String |  |
| response | success | String | Success or Fail |
| * status idle cueing cue\_done play pause | true  false  false  false  false | Boolean  Boolean  Boolean  Boolean  Boolean | Not doing anything or stopped  Preparing play or record  Completed prepare play or record  Playing scroll  Paused scroll |

* **get\_rate**The [get\_rate] command get current play rate.  
    
  {   
   “command” : “get\_rate”  
  }  
    
  **Response**

|  |  |  |  |
| --- | --- | --- | --- |
| **JSON Object** | **JSON Value** | **Value Type** | **Description** |
| command | get\_timecode | String |  |
| response | success | String | Success or Fail |
| rate | 0 | Number (float) | 0 : pause  Greater then 0 : forward scroll  Less then 0 : rewind scroll |

1. **Logo**

**System Control**

* **open**Open to use device.  
  No other commands can be executed before this command is executed.  
    
  {   
   “command” : “open”  
  }
* **close**  
  Close the device.  
  No other commands can be executed after this command.  
    
  {   
   “command” : “close”  
  }

**Immediate Control**

* **stop**The [stop] command stops display logo. (logo off)  
  {   
   “command” : “stop”  
  }
* **play**Start playback display logo. (logo on)
* Play Cue before you start playback logo.

{   
 “command” : “play”  
}

**Preset/Select Control**

* **play\_cue**The [play\_cue] command prepares for playback display logo.  
  If the logo ID is not found, an error occurs and state returns STOP.  
  When the CUE is complete, the CUE-DONE flag is set in status.

|  |  |  |  |
| --- | --- | --- | --- |
| **JSON Object** | **JSON Value** | **Value Type** | **Description** |
| command | play\_cue | String |  |
| id | id | String | Logo ID |

{   
 “command” : “play\_cue”,  
 “id” : “id”  
}

**Sense Request**

* **get\_device\_no**The [get\_device\_no] command get device number.  
    
  {   
   “command” : “get\_device\_no”  
  }  
    
  **Response**

|  |  |  |  |
| --- | --- | --- | --- |
| **JSON Object** | **JSON Value** | **Value Type** | **Description** |
| command | get\_device\_no | String |  |
| response | success | String | Success or Fail |
| no | 0 | Number | Get PCS the set device number. |

* **get\_status**The [get\_status] command get device status.  
    
  {   
   “command” : “get\_status”  
  }  
    
  **Response**

|  |  |  |  |
| --- | --- | --- | --- |
| **JSON Object** | **JSON Value** | **Value Type** | **Description** |
| command | get\_status | String |  |
| response | success | String | Success or Fail |
| * status idle  cueing cue\_done play | True  false  false  false | Boolean  Boolean  Boolean  Boolean | Not doing anything or stopped (logo off)  Preparing display logo  Completed prepare logo  Playing logo (logo on) |

1. **Closed Caption & Sub Title**

**System Control**

* **open**Open to use device.  
  No other commands can be executed before this command is executed.  
    
  {   
   “command” : “open”  
  }
* **close**  
  Close the device.  
  No other commands can be executed after this command.  
    
  {   
   “command” : “close”  
  }

**Immediate Control**

* **stop**The [stop] command stops playback.  
    
  {   
   “command” : “stop”  
  }
* **play**Start playback.  
  If the decoder in PAUSE state, the [play] command start playback at current position.  
  If the decoder in ON state, then open caption.  
  If the decoder not in ON state, then closed caption.
* Play Cue before you start playback.

{   
 “command” : “play”  
}

* **pause**The [pause] command pause playback.  
  If the device in PLAY or PLAY CUE state, the [pause] command causes the currently playing ID to pause and if device in ON then display a caption.  
    
  {   
   “command” : “pause”  
  }
* **set\_on**Specifies the display caption on screen.

|  |  |  |  |
| --- | --- | --- | --- |
| **JSON Object** | **JSON Value** | **Value Type** | **Description** |
| command | set\_on | String |  |
| on | true | Boolean | true : Display caption  false : Hide caption, only in video signal |

{   
 “command” : “set\_on”,  
 “on” : true  
}

**Preset/Select Control**

* **play\_cue**The [play\_cue] command prepares for playback.  
  If the ID is not found, an error occurs and state returns STOP.  
  When the CUE is complete, the CUE-DONE flag is set in status.

|  |  |  |  |
| --- | --- | --- | --- |
| **JSON Object** | **JSON Value** | **Value Type** | **Description** |
| command | play\_cue | String |  |
| id | id | String | Preset or smi |

{   
 “command” : “play\_cue”,  
 “id” : “id”  
}

* **play\_cue\_data**Performs similar to [play\_cue].  
  In addition, you can specify playback start timecode and playback duration.

|  |  |  |  |
| --- | --- | --- | --- |
| **JSON Object** | **JSON Value** | **Value Type** | **Description** |
| command | play\_cue\_data | String |  |
| id | id | String | Preset or smi |
| start | 00:00:00:00 | String | Playback start timecode |
| duration | 00:59:59:29 | String | Playback duration timecode |

{   
 “command” : “play\_cue\_data”,  
 “id” : “id”,  
 “start” : “00:00:00:00”,  
 “duration” : “00:59:59:29”  
}

**Sense Request**

* **get\_device\_no**The [get\_device\_no] command get device number.  
    
  {   
   “command” : “get\_device\_no”  
  }  
    
  **Response**

|  |  |  |  |
| --- | --- | --- | --- |
| **JSON Object** | **JSON Value** | **Value Type** | **Description** |
| command | get\_device\_no | String |  |
| response | success | String | Success or Fail |
| no | 0 | Number | Get PCS the set device number. |

* **get\_status**The [get\_status] command get device status.  
    
  {   
   “command” : “get\_status”  
  }  
    
  **Response**

|  |  |  |  |
| --- | --- | --- | --- |
| **JSON Object** | **JSON Value** | **Value Type** | **Description** |
| command | get\_status | String |  |
| response | success | String | Success or Fail |
| * status idle cueing cue\_done play pause on | true  false  false  false  false  false | Boolean  Boolean  Boolean  Boolean  Boolean  Boolean | Not doing anything or stopped  Preparing play or record  Completed prepare play or record  Playing  Paused  Display caption on/off |

* **get\_timecode**The [get\_timecode] command get current timecode.  
    
  {   
   “command” : “get\_timecode”  
  }  
    
  **Response**

|  |  |  |  |
| --- | --- | --- | --- |
| **JSON Object** | **JSON Value** | **Value Type** | **Description** |
| command | get\_timecode | String |  |
| response | success | String | Success or Fail |
| timecode | 00:00:00:00 | String |  |

1. **MCS – Master Control Switch**

**System Control**

* **open**Open to use device.  
  No other commands can be executed before this command is executed.  
    
  {   
   “command” : “open”  
  }
* **close**  
  Close the device.  
  No other commands can be executed after this command.  
    
  {   
   “command” : “close”  
  }

**Immediate Control**

* **next\_transition**The [next\_transition] command sets the next transition of the background or key.

|  |  |  |  |
| --- | --- | --- | --- |
| **JSON Object** | **JSON Value** | **Value Type** | **Description** |
| command | next\_transition | String |  |
| background | true | Boolean | Background selected |
| key | true | Boolean | Keyers selected |

{   
 “command” : “next\_tranition”  
 “background” : “true”,  
 “key” : “true”  
}

* **start\_transition**The start of the next transition.
* Next Transition before you start transition.

{   
 “command” : “start\_transition”  
}

* **crosspoint\_take**This command set crosspoint take.  
  The [crosspoint\_take] command will clear any overs that may be selected.  
  The number of bus parameter can be change.

|  |  |  |  |
| --- | --- | --- | --- |
| **JSON Object** | **JSON Value** | **Value Type** | **Description** |
| command | crosspoint\_take | String |  |
| * bus program preset output1 output2 | true true true true | Boolean Boolean Boolean Boolean | Select program bus Select preset bus Select output1 Select output2 |
| crosspoint | 0 | Number (integer) | 0 : No change  1~16 : Crosspoint number (Device number) |

{   
 “command” : “crosspoint\_take”,  
 “bus” : {  
 “program” : true,  
 “preset” : true,  
 “output1” : true,  
 “output2” : true  
 },  
 “crosspoint” : 0  
}

* **key\_assign**This command assign key to bus.  
  The [key\_assign] command the key use to PGM or PST or output.  
  The number of key parameter can be change.

|  |  |  |  |
| --- | --- | --- | --- |
| **JSON Object** | **JSON Value** | **Value Type** | **Description** |
| command | key\_take | String |  |
| * keys key1 key2 key3 key4 key5 key6 key7 key8 | program program preset preset output1 none output2 none | String String String String String String String String | Set the bus name. (program, preset, output1, output2) |

{   
 “command” : “key\_take”,  
 “keys” : {  
 “key1” : program,  
 “key2” : program,  
 “key3” : preset,  
 “key4” : preset,  
 “key5” : output1,  
 “key6” : none,  
 “key7” : output2,  
 “key8” : none  
 }  
}

* **key\_take**This command set key take.  
  The [key\_take] command turns the key on/off.  
  The number of key parameter can be change.

|  |  |  |  |
| --- | --- | --- | --- |
| **JSON Object** | **JSON Value** | **Value Type** | **Description** |
| command | key\_take | String |  |
| * keys key1 key2 key3 key4 key5 key6 key7 key8 | true true true true true true true true | Boolean Boolean Boolean Boolean Boolean Boolean Boolean Boolean | Set the key turns on/off. |

{   
 “command” : “key\_take”,  
 “keys” : {  
 “key1” : true,  
 “key2” : true,  
 “key3” : true,  
 “key4” : true,  
 “key5” : true,  
 “key6” : true,  
 “key7” : true,  
 “key8” : true  
 }  
}

**Preset/Select Control**

* **set\_transition\_type**This command set transition type.

|  |  |  |  |
| --- | --- | --- | --- |
| **JSON Object** | **JSON Value** | **Value Type** | **Description** |
| command | set\_transition\_type | String |  |
| type | cut | String | cut  fade-fade  cut-fade  mix  fade-cut |

{   
 “command” : “set\_transition\_type”,  
 “type” : “cut”  
}

* **set\_transition\_rate**This command set transition rate.

|  |  |  |  |
| --- | --- | --- | --- |
| **JSON Object** | **JSON Value** | **Value Type** | **Description** |
| command | set\_transition\_rate | String |  |
| rate | slow | String | slow,  medium,  fast,  rate : 0 ~ 65535 frames |

{   
 “command” : “set\_transition\_rate”,  
 “rate” : “slow”  
}

* **set\_enable\_key**This command set enable key.  
  The [set\_enable\_key] command sets whether the key is transited together during transition.  
  Key can be assigned only CG (Cut & Page), Sequence CG, Scroll CG, Logo, Closed Caption & Sub Title devices. Allocate devices from the PCS.

|  |  |  |  |
| --- | --- | --- | --- |
| **JSON Object** | **JSON Value** | **Value Type** | **Description** |
| command | set\_enable\_key | String |  |
| * keys key1 key2 key3 key4 key5 key6 key7 key8 | true true true true true true true true | Boolean Boolean Boolean Boolean Boolean Boolean Boolean Boolean | Set the key enable. |

{   
 “command” : “set\_enable\_key”,  
 “keys” : {  
 “key1” : true,  
 “key2” : true,  
 “key3” : true,  
 “key4” : true,  
 “key5” : true,  
 “key6” : true,  
 “key7” : true,  
 “key8” : true  
 }  
}

**Sense Request**

* **get\_transition\_type**The [get\_transition type] command get currently set the transition type.  
    
  {   
   “command” : “get\_transition\_type”  
  }  
    
  **Response**

|  |  |  |  |
| --- | --- | --- | --- |
| **JSON Object** | **JSON Value** | **Value Type** | **Description** |
| command | get\_transition\_type | String |  |
| response | success | String | Success or Fail |
| type | cut | String | cut  fade-fade  cut-fade  mix  fade-cut |

* **get\_transition\_rate**The [get\_transition\_rate] command get currently set the transition rate.  
    
  {   
   “command” : “get\_transition\_rate”  
  }  
    
  **Response**

|  |  |  |  |
| --- | --- | --- | --- |
| **JSON Object** | **JSON Value** | **Value Type** | **Description** |
| command | get\_transition\_rate | String |  |
| response | success | String | Success or Fail |
| rate | slow | String | slow,  medium,  fast,  rate : 0 ~ 65535 frames |

* **get\_crosspoint\_take**The [get\_crosspoint\_take] command get currently set the crosspoint take information.

|  |  |  |  |
| --- | --- | --- | --- |
| **JSON Object** | **JSON Value** | **Value Type** | **Description** |
| command | get\_crosspoint\_take | String |  |

{   
 “command” : “get\_crosspoint\_take”  
}  
  
**Response**

|  |  |  |  |
| --- | --- | --- | --- |
| **JSON Object** | **JSON Value** | **Value Type** | **Description** |
| command | get\_crosspoint\_take | String |  |
| response | success | String | Success or Fail |
| program | 1 | Number  (integer) | 1~16 : Crosspoint number (Device number) |
| preset | 2 |
| output1 | 3 |
| output2 | 4 |

* **get\_enable\_key**The [get\_enable\_key] command get currently key enable information.

|  |  |  |  |
| --- | --- | --- | --- |
| **JSON Object** | **JSON Value** | **Value Type** | **Description** |
| command | get\_enable\_key | String |  |

{   
 “command” : “get\_enable\_key”

}  
  
**Response**

|  |  |  |  |
| --- | --- | --- | --- |
| **JSON Object** | **JSON Value** | **Value Type** | **Description** |
| command | get\_enable\_key | String |  |
| response | success | String | Success or Fail |
| * keys key1 key2 key3 key4 key5 key6 key7 key8 | true true true true true true true true | Boolean Boolean Boolean Boolean Boolean Boolean Boolean Boolean | Get the key enable information. |

* **get\_key\_assign**The [get\_key\_assign] command get key assigned bus.  
    
  {   
   “command” : “get\_key\_assign”  
  }  
    
  **Response**

|  |  |  |  |
| --- | --- | --- | --- |
| **JSON Object** | **JSON Value** | **Value Type** | **Description** |
| command | get\_key\_take | String |  |
| response | success | String | Success or Fail |
| * status key1 key2 key3 key4 key5 key6 key7 key8 | program program preset preset output1 none output2 none | String String String String String String String String | Set the bus name. (program, preset, output1, output2, none) |

* **get\_key\_take**The [get\_key\_take] command get key on/off status.  
    
  {   
   “command” : “get\_key\_take”  
  }  
    
  **Response**

|  |  |  |  |
| --- | --- | --- | --- |
| **JSON Object** | **JSON Value** | **Value Type** | **Description** |
| command | get\_key\_take | String |  |
| response | success | String | Success or Fail |
| * status key1 key2 key3 key4 key5 key6 key7 key8 | true true true true true true true true | Boolean Boolean Boolean Boolean Boolean Boolean Boolean Boolean | Get the key on/off information. |

* **get\_status**The [get\_status] command get device status.  
    
  {   
   “command” : “get\_status”  
  }  
    
  **Response**

|  |  |  |  |
| --- | --- | --- | --- |
| **JSON Object** | **JSON Value** | **Value Type** | **Description** |
| command | get\_status | String |  |
| response | success | String | Success or Fail |
| status | quiescent | String | quiescent, transitional, fadingtoblack, fadingfromblack, inblack |