* **Explanation of simultaneous control error of two or more media devices by communication (Control by SEC**)

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| NO | Command | Media1 layer output | Media1 device status | Media2 layer output | Media2 device status |
| 1 | Initial state | black | idle | black | idle |
| 2 | play\_cue file1 | file1 first or in point frame | 1. idle  2. cue  3. paused & cue\_done | file1 first or in point frame | 1. idle  2. cue  3. paused & cue\_done |
| 3 | play | file1 playback | playing | file1 playback | playing |
| 4 | play\_cue file2 | file1 playback | 1. playing & cue  2. playing & cue\_done | file1 playback | 1. playing & cue  2. playing & cue\_done |
| 5 | play | file1 playback | playing | file2 playback | playing |
| 6 | play\_cue file3 | file3 playback | playing | file2 playback | 1. playing & cue  2. playing & cue\_done  3. playing |
| 7 | play | file3 playback | playing | file3 playback | playing |
| 8 | play\_cue file4 | file4 playback | playing | file3 playback | 1. playing & cue  2. playing & cue\_done  3. playing |
| 9 | Play | file4 playback | playing | file4 playback | playing |
| 10 | play\_cue file5 | file5 playback | playing | file4 playback | 1. playing & cue  2. playing & cue\_done  3. playing |
| 11 | Play | file5 playback | playing | file5 playback | playing |
| . | . | . | . | . | . |